Lab 4 mini instructions.

In this practice we are going to build a resettable counter that will display on the red leds how many times any of the push-buttons are pushed and can be reset when slider switch zero (first switch) is up and a button is pushed and released. Some interesting reading about switch bouncing can be found at this site <http://www.ganssle.com/debouncing.htm> it may help you understand why one part of the lab is needed.